{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Ark1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,4],[3,1,3,3]]}
["RESIN BEREGNING"]
[null,"INDTAST HERUNDER",null,"INDTAST HERUNDER"]
["Indtast resin i alt:",null,"liter",null,"kg"]
[]
["Resin i alt:",{"$f":"IF(ISNUMBER(B3), B3, D3/1.3514)","v":0},"liter",{"$f":"IF(ISNUMBER(B3), B3 * 1.3514, B5*1.3514)","v":0},"kg"]
["Harpiks (B)",{"$f":"B5/3*2","v":0},"liter",{"$f":"B6*1.252","v":0},"kg"]
["Vandglas (A)",{"$f":"B5/3","v":0},"liter",{"$f":"B7*1.55","v":0},"kg"]